Graphtec Cutting Plotter Driver OPS662 Ver.3.00
for Microsoft Windows Vista / Windows 7 / Windows 8 / Windows 8.1 / Windows 10

Thank you for choosing the Graphtec OPS662 Cutting Plotter Driver. 

The README.TXT file in each directory contains instructions on installation and
operation as well as other notes. Be sure to read them carefully before 
installing or using this driver.

Before you begin installation, check that the program disk contains the 
following:
      GDSETUP.EXE
      GDSETUP.INI

      WIN_X86\DISK1            For Windows Vista/7/8/8.1/10
      WIN_X86\GPCUT.DLL
      WIN_X86\GPCUTUI.DLL
      WIN_X86\GPCUTUI.CHM
      WIN_X86\GPCUTMON.DLL
      WIN_X86\GPCUT.INF
      WIN_X86\GPCUT.CAT
      WIN_X86\README.TXT
      WIN_X86\CE30MK2.GPD
      WIN_X86\FC7000.GPD
      WIN_X86\FC2240.GPD
      WIN_X86\CE5000.GPD
      WIN_X86\FC2250.GPD
      WIN_X86\FC8000.GPD
      WIN_X86\FC4500.GPD
      WIN_X86\CE6000.GPD
      WIN_X86\FC8600.GPD


Required PC specifications
(The specification needs to be higher than recommended specification
 by using OS)

* OS           : Windows Vista
                  (Home Basic, Home Premium, Business, Enterprise, Ultimate)
                 Windows 7
                  (Home Basic, Home Premium, Professional, Enterprise, Ultimate)
                 Windows 8
                  (Windows 8, Pro, Enterprise)
                 Windows 8.1
                  (Windows 8.1, Pro, Enterprise)
                 Windows 10
                  (Home, Pro, Enterprise, Education)
* CPU          : Pentium 4 / AMD Athlon 64 800MHz or faster
* Memory       : 1GB or larger
* Display      : 1024x768 True Color
* Mouse
* CD-ROM drive
* Network interface  : 10Base-T/100Base-TX
* USB interface      : USB2.0(Full Speed)
* Serial interface   : RS-232C
* Parallel interface : Centronics parallel interface
Note:
 The interface which can be used depends on the plotter model.
 The plotter needs to be connected with either interface.


Precautions to be observed when connecting the Graphtec Cutting Plotter 
via USB.
   * Operation with other than the included driver is not guaranteed.
   * Do not connect multiple plotters to a single computer.
   * Operation is not guaranteed if the plotter is connected to a USB hub 
     or to a USB extension board.

END
